(footprint "PEC12R-4xxxF-Sxxxx"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -9.5 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "ac48072e-6222-49b3-85f2-987d83bde50d")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "PEC12R-4xxxF-Sxxxx"
		(at 0 -14 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "225b39d6-36aa-458c-9cd7-d5f4eecc9e4c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "PEC12R-4xxxF-Sxxxx"
		(at 0 13 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "49e4e3f6-926f-4301-af52-bd794c37cdc2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "7c4a6735-3ecb-42f4-9da9-e65e1734f8c8")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" "Rotary Encoder with Push-Button Switch"
		(at 0 11.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "19ea83fa-4546-4299-bfdd-acb9b9a23125")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr through_hole)
	(fp_line
		(start -6.6 -2)
		(end -6.6 -7)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e5db5737-9a57-44b5-b524-a9a3e91bb404")
	)
	(fp_line
		(start -6.6 2)
		(end -6.6 7.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "934d4eee-578e-431f-b807-8a4b6dccc67d")
	)
	(fp_line
		(start -6.5 -7)
		(end -4 -7)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "fd03e324-f206-4c41-8ada-fd9466cecfd7")
	)
	(fp_line
		(start -6.5 7.5)
		(end -4 7.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "62dabbbc-9ff6-407d-9829-8af3c951065f")
	)
	(fp_line
		(start 4 -7)
		(end 6.5 -7)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "a8fbc71f-3ec1-4217-99fa-947a68f2941b")
	)
	(fp_line
		(start 4 7.5)
		(end 6.5 7.5)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "f3efd156-15c5-4928-bc90-df41f47c1881")
	)
	(fp_line
		(start 6.6 -7)
		(end 6.6 -2)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "e0cd1d24-d705-4a64-994c-e76e7c7d0c70")
	)
	(fp_line
		(start 6.6 7.5)
		(end 6.6 2)
		(stroke
			(width 0.2)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "c43fa126-776f-4830-9041-448ee8f2d3ff")
	)
	(fp_text user "${REFERENCE}"
		(at 0 10 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "bbdca5bd-ace6-47f6-8858-c879d4d64c8c")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "" np_thru_hole oval
		(at -6.6 0)
		(size 3 3.3)
		(drill oval 2 2.3)
		(layers "F&B.Cu" "*.Mask")
		(uuid "a870c822-143e-4d4e-900c-e78dea75ffdd")
	)
	(pad "" np_thru_hole oval
		(at 6.6 0)
		(size 3 3.3)
		(drill oval 2 2.3)
		(layers "F&B.Cu" "*.Mask")
		(uuid "db76a0de-5cf6-4bf1-be92-460cb788b013")
	)
	(pad "1" thru_hole circle
		(at -2.5 -7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "60a1b19c-4ec1-4ffc-80de-67b3b6ca5edf")
	)
	(pad "2" thru_hole circle
		(at 2.5 -7)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "6aa9bbdf-ce9a-4385-b51b-265416b13c46")
	)
	(pad "A" thru_hole circle
		(at -2.5 7.5)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "241eb4f1-8088-440a-8de0-5447a1bd345d")
	)
	(pad "B" thru_hole circle
		(at 2.5 7.5)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "2b49e791-0073-410e-82a2-25f5206971ff")
	)
	(pad "C" thru_hole circle
		(at 0 7.5)
		(size 1.524 1.524)
		(drill 0.762)
		(layers "*.Cu" "*.Mask")
		(remove_unused_layers no)
		(uuid "b0e38661-15f4-4fe4-b07b-02e2eb64b871")
	)
)
