(footprint "TS-1101-C-W Button"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(property "Reference" "REF**"
		(at 0 -3 0)
		(unlocked yes)
		(layer "F.SilkS")
		(uuid "5fe641d6-628a-46bd-89e0-57cc380a60eb")
		(effects
			(font
				(size 1 1)
				(thickness 0.1)
			)
		)
	)
	(property "Value" "TS-1101-C-W Button"
		(at 0 4.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "cba93b73-f249-4e61-8445-9dad12a81424")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Footprint" "TS-1101-C-W Button"
		(at 0 6.5 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "bac33d84-b86d-46d9-8004-519cafa7a039")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "1874b105-4780-4204-a80b-cc4065f51f0f")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
		(uuid "94929be7-18bf-4a94-88f8-82fd9a3b96c2")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(attr smd)
	(fp_line
		(start -2.2 -1.8)
		(end 0 -1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "0d603692-fde0-4044-9005-b8b04cf111e8")
	)
	(fp_line
		(start -2.2 1.8)
		(end 0 1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "34d912d8-14b6-4d0e-acc2-2dca1694961f")
	)
	(fp_line
		(start 2.2 -1.8)
		(end 0 -1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "5e57607a-b145-4afe-89d9-37539add9aed")
	)
	(fp_line
		(start 2.2 1.8)
		(end 0 1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "33f1a18e-257a-4a39-aaef-797d282e1cfd")
	)
	(fp_rect
		(start -1 -0.5)
		(end 1 0.5)
		(stroke
			(width 0.1)
			(type default)
		)
		(fill none)
		(layer "F.SilkS")
		(uuid "a2d1b736-e51d-4d8f-9735-5c7049a82e15")
	)
	(fp_arc
		(start -3 -1)
		(mid -2.765685 -1.565685)
		(end -2.2 -1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "4f48f694-b404-4703-b422-f57b69cde588")
	)
	(fp_arc
		(start -2.2 1.8)
		(mid -2.765685 1.565685)
		(end -3 1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "57ae014e-0b94-4805-ade7-1fabb86197a8")
	)
	(fp_arc
		(start 2.2 -1.8)
		(mid 2.765685 -1.565685)
		(end 3 -1)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "1aedb683-c49a-4c82-b1cf-c32e394964ed")
	)
	(fp_arc
		(start 3 1)
		(mid 2.765685 1.565685)
		(end 2.2 1.8)
		(stroke
			(width 0.1)
			(type default)
		)
		(layer "F.SilkS")
		(uuid "ed65f769-773d-413e-a907-8063173d6682")
	)
	(fp_text user "${REFERENCE}"
		(at 0 6 0)
		(unlocked yes)
		(layer "F.Fab")
		(uuid "4d4a37a1-0f2b-4453-8a01-f237537e835a")
		(effects
			(font
				(size 1 1)
				(thickness 0.15)
			)
		)
	)
	(pad "1" smd rect
		(at 3.7 0)
		(size 1.2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "3897ac84-c975-4cae-9a4b-bee3e51d5878")
	)
	(pad "2" smd rect
		(at -3.7 0)
		(size 1.2 1)
		(layers "F.Cu" "F.Paste" "F.Mask")
		(uuid "ce2ce015-0c79-46be-bf03-ec31074d4a15")
	)
)
